Gemstone Communication Library
Show/Hide TOC

# UdpClientAllowDualStackSocket Property

Gets or sets a boolean value that determines if dual-mode socket is allowed when endpoint address is IPv6.

## Definition

Namespace: Gemstone.Communication
Assembly: Gemstone.Communication (in Gemstone.Communication.dll) Version: 1.0.177 -- Release Build+8887b83d11297810a428ddc908af248f40f0d268
C#
View Source Request Example

    public bool AllowDualStackSocket { get; set; }

VB
View Source Request Example

    Public Property AllowDualStackSocket As Boolean
    	Get
    	Set

C++
View Source Request Example

    public:
    property bool AllowDualStackSocket {
    	bool get ();
    	void set (bool value);
    }

JavaScript
View Source Request Example

    function get_AllowDualStackSocket();
    function set_AllowDualStackSocket(value);

#### Property Value

Boolean

## See Also

#### Reference

UdpClient Class
Gemstone.Communication Namespace