Gemstone PhasorProtocols Library
Show/Hide TOC

# CommonFrameHeader Properties

## Properties

AsduCount | Gets or sets number of ASDUs in this frame.
AsduLength | Gets or sets ASDU length in this frame.
BinaryImage | Gets the binary image of the common header portion of this frame.
ConfigurationFrame | Gets or sets current configuration frame.
ConfigurationRevision | Gets or sets configuration revision;
DataLength | Gets or sets the length of the data in the IEC 61850-90-5 frame (i.e., the FrameLength minus the header length and checksum: FrameLength - 8).
FractionOfSecond | Gets the IEC 61850-90-5 fraction of second.
FrameLength | Gets or sets the IEC 61850-90-5 frame length of this frame.
FrameType | Gets the fundamental frame type of this frame.
GuessConfiguration | Gets or sets flag that determines if system should try to guess at a possible configuration given payload size.
IDCode | Gets or sets the IEC 61850-90-5 ID code of this frame.
IgnoreSampleSizeValidationFailures | Gets or sets flag that determines if system should ignore sample size validation errors.
IgnoreSignatureValidationFailures | Gets or sets flag that determines if system should ignore checksum signature validation errors.
KeyID | Gets or sets key ID - lookup into table of current keys.
Length | Gets the IEC 61850-90-5 frame header length.
MsvID | Gets or sets the MSVID to be used by IEC 61850-90-5 data frames.
PacketNumber | Gets or sets packet number of this frame.
ParseRedundantASDUs | Gets or sets flag that determines if system should expose redundantly parsed ASDUs.
PhasorAngleFormat | Gets or sets the AngleFormat for the IPhasorDefinition objects.
PublishFrame | Gets or sets delegate to method used to publish new frames.
SecondOfCentury | Gets the IEC 61850-90-5 second of century.
SecurityAlgorithm | Gets or sets security algorithm used by IEC61850-90-5 data frames.
SignatureAlgorithm | Gets or sets signature algorithm used by IEC61850-90-5 data frames.
SpduLength | Gets SPDU length.
State | Gets or sets the parsing state for the CommonFrameHeader object.
Timebase | Gets or sets the IEC 61850-90-5 resolution of fractional time stamps.
TimeQualityFlags | Gets or sets the IEC 61850-90-5 TimeQualityFlags.
TimeQualityIndicatorCode | Gets or sets the IEC 61850-90-5 TimeQualityIndicatorCode.
Timestamp | Gets or sets timestamp of this CommonFrameHeader.
TimeTag | Gets time as a UnixTimeTag representing seconds of current Timestamp.
TypeID | Gets or sets the IEC 61850-90-5 specific frame type of this frame.
UseETRConfiguration | Gets or sets flag that determines if system should find associated ETR file using MSVID with same name for configuration.
Version | Gets or sets the IEC 61850-90-5 version of this frame.

## See Also

#### Reference

CommonFrameHeader Class
Gemstone.PhasorProtocols.IEC61850_90_5 Namespace