Gemstone Timeseries Library
Show/Hide TOC

# InputAdapterBase Properties

## Properties

AutoStart | Gets or sets flag indicating if adapter should automatically start or otherwise connect on demand. (Inherited from AdapterBase)
ConnectionAttemptInterval | Gets or sets the connection attempt interval, in milliseconds, for the data input source.
ConnectionInfo | Gets connection info for adapter, if any. (Inherited from AdapterBase)
ConnectionString | Gets or sets key/value pair connection information specific to this AdapterBase. (Inherited from AdapterBase)
DataSource | Gets or sets DataSet based data source available to this AdapterBase. (Inherited from AdapterBase)
EnableConnectionErrors | When false, connection errors do not get logged through OnProcessException. When true, connection errors will be logged normally.
Enabled | Gets or sets enabled state of this AdapterBase. (Inherited from AdapterBase)
ID | Gets or sets numeric ID associated with this AdapterBase. (Inherited from AdapterBase)
InitializationTimeout | Gets or sets maximum time system will wait during Start for initialization. (Inherited from AdapterBase)
Initialized | Gets or sets flag indicating if the adapter has been initialized successfully. (Inherited from AdapterBase)
InputMeasurementKeys | Gets or sets primary keys of input measurements the AdapterBase expects, if any.
IsConnected | Gets flag that determines if InputAdapterBase is connected.
IsDisposed | Gets a flag that indicates whether the object has been disposed. (Inherited from AdapterBase)
Log | Log messages generated by an adapter. (Inherited from AdapterBase)
MeasurementReportingInterval | Gets or sets the measurement reporting interval. (Inherited from AdapterBase)
Name | Gets or sets the name of this AdapterBase. (Inherited from AdapterBase)
OutputMeasurements | Gets or sets output measurements that the AdapterBase will produce, if any. (Inherited from AdapterBase)
OutputSourceIDs | Gets or sets Source values used to filter output measurements.
ProcessedMeasurements | Gets the total number of measurements handled thus far by the AdapterBase. (Inherited from AdapterBase)
ProcessingInterval | Gets or sets the desired processing interval, in milliseconds, for the adapter. (Inherited from AdapterBase)
RequestedOutputMeasurementKeys | Gets or sets output measurement keys that are requested by other adapters based on what adapter says it can provide.
RunTime | Gets the total amount of time, in seconds, that the adapter has been active. (Inherited from AdapterBase)
Settings | Gets settings DictionaryTKey, TValue parsed when ConnectionString was assigned. (Inherited from AdapterBase)
StartTime | Gets the UTC time this AdapterBase was started. (Inherited from AdapterBase)
StartTimeConstraint | Gets the start time temporal processing constraint defined by call to SetTemporalConstraint(String, String, String). (Inherited from AdapterBase)
Status | Returns the detailed status of the data input source. (Overrides AdapterBaseStatus)
StopTime | Gets the UTC time this AdapterBase was stopped. (Inherited from AdapterBase)
StopTimeConstraint | Gets the stop time temporal processing constraint defined by call to SetTemporalConstraint(String, String, String). (Inherited from AdapterBase)
SupportsTemporalProcessing | Gets the flag indicating if this adapter supports temporal processing. (Inherited from AdapterBase)
UseAsyncConnect | Gets flag that determines if the data input connects asynchronously.

## See Also

#### Reference

InputAdapterBase Class
Gemstone.Timeseries.Adapters Namespace