Gemstone PhasorProtocols Library
Show/Hide TOC

# ConfigurationFrame Properties

## Properties

AllowQueuedPublication | Gets flag that determines if frame image can be queued for publication or should be processed immediately. (Inherited from ConfigurationFrameBase)
Attributes | DictionaryTKey, TValue of string based property names and values for the ConfigurationFrame object. (Overrides ConfigurationFrameBaseAttributes)
BinaryImage | Gets the binary image of this ChannelFrameBaseT. (Inherited from ChannelFrameBaseT)
BinaryLength | Gets the length of the ConfigurationFrame. (Overrides ChannelFrameBaseT BinaryLength)
BodyImage | Gets the binary body image of this ChannelFrameBaseT. (Inherited from ChannelFrameBaseT)
BodyLength | Gets the length of the BodyImage. (Inherited from ChannelFrameBaseT)
Cells | Gets reference to the ConfigurationCellCollection for this ConfigurationFrame.
Checksum | Gets calculated checksum for this ChannelFrameBaseT. (Inherited from ChannelFrameBaseT)
CommonHeader | Gets or sets current CommonFrameHeader.
ConfigurationFileName | Gets the INI based configuration file name of this ConfigurationFrame.
CreatedTimestamp | Gets timestamp, in ticks, of when this ChannelFrameBaseT was created. (Inherited from ChannelFrameBaseT)
DataFrameLength | Gets length of data frame based on enabled streaming data.
DefaultFrequency | Gets the default frequency definition.
DefaultPhasorI | Gets the default current phasor definition.
DefaultPhasorV | Gets the default voltage phasor definition.
Digital1Included | Gets flag that determines if Digital 1 is included in ON-LINE data.
Digital2Included | Gets flag that determines if Digital 2 is included in ON-LINE data.
FooterImage | Gets the binary footer image of the BinaryImageBase object. (Inherited from ChannelBase)
FooterLength | Gets the length of the footer portion of the BinaryImageBase object. (Inherited from BinaryImageBase)
FrameRate | Gets or sets defined frame rate of this ConfigurationFrameBase. (Inherited from ConfigurationFrameBase)
FrameType | Gets the FundamentalFrameType for this ConfigurationFrameBase. (Inherited from ConfigurationFrameBase)
HeaderImage | Gets the binary header image of the DataFrame object. (Overrides ChannelBaseHeaderImage)
HeaderLength | Gets the length of the HeaderImage. (Overrides HeaderLength)
IDCode | Gets or sets the numeric ID code for this ConfigurationCell. (Overrides ChannelFrameBaseT IDCode)
LastSortedMeasurement | Gets or sets reference to last IMeasurement that was sorted into this ChannelFrameBaseT. (Inherited from ChannelFrameBaseT)
Lifespan | Gets the life-span of this ChannelFrameBaseT since its creation. (Inherited from ChannelFrameBaseT)
Measurements | Keyed measurements in this ChannelFrameBaseT. (Inherited from ChannelFrameBaseT)
OnlineDataFormatFlags | Gets or sets the Macrodyne OnlineDataFormatFlags of this ConfigurationFrame.
ParsedBinaryLength | Gets the parsed binary length derived from the parsing state, if any. (Inherited from ChannelFrameBaseT)
PhasorCount | Gets phasor count derived from OnlineDataFormatFlags of this ConfigurationFrame.
Published | Gets or sets published state of this ChannelFrameBaseT. (Inherited from ChannelFrameBaseT)
ReferenceIncluded | Gets flag that determines if reference phasor is included in ON-LINE data.
SortedMeasurements | Gets or sets total number of measurements that have been sorted into this ChannelFrameBaseT. (Inherited from ChannelFrameBaseT)
Source | Gets or sets the data source identifier for this ChannelFrameBaseT. (Inherited from ChannelFrameBaseT)
State | Gets or sets the parsing state for the this ConfigurationFrameBase. (Inherited from ConfigurationFrameBase)
StationName | Gets station name retrieved from header frame.
Status2Included | Gets flag that determines if status 2 flags are included in ON-LINE data.
Tag | Gets or sets a user definable reference to an object associated with this ChannelBase object. (Inherited from ChannelBase)
TicksPerFrame | Gets the defined Ticks per frame of this ConfigurationFrameBase. (Inherited from ConfigurationFrameBase)
Timestamp | Gets or sets exact timestamp, in ticks, of the data represented by this ChannelFrameBaseT. (Inherited from ChannelFrameBaseT)
TimestampIncluded | Gets flag that determines if timestamp is included in ON-LINE data.
TimeTag | Gets UNIX based time representation of the ticks of this ChannelFrameBaseT. (Inherited from ChannelFrameBaseT)
TrustHeaderLength | Gets or sets flag that determines if header lengths should be trusted over parsed byte count. (Inherited from ChannelFrameBaseT)
TypeID | Gets the identifier that is used to identify the Macrodyne frame.
ValidateCheckSum | Gets or sets flag that determines if frame's check-sum should be validated - this should normally be left as true. (Inherited from ChannelFrameBaseT)

## See Also

#### Reference

ConfigurationFrame Class
Gemstone.PhasorProtocols.Macrodyne Namespace