Gemstone PhasorProtocols Library
Show/Hide TOC

# ConfigurationCell Properties

## Properties

AnalogDataFormat | Gets or sets the DataFormat for the IAnalogDefinition objects in the AnalogDefinitions of this ConfigurationCell. (Overrides ConfigurationCellBaseAnalogDataFormat)
AnalogDefinitions | Gets a reference to the AnalogDefinitionCollection of this ConfigurationCellBase. (Inherited from ConfigurationCellBase)
Attributes | DictionaryTKey, TValue of string based property names and values for the ConfigurationCell object. (Overrides ConfigurationCellBaseAttributes)
AutoPadIDLabelImage | Gets flag that indicates if IDLabelImage should auto pad-right value to IDLabelLength. (Inherited from ConfigurationCellBase)
AutoPadStationNameImage | Gets flag that indicates if StationNameImage should auto pad-right value to MaximumStationNameLength. (Inherited from ConfigurationCellBase)
BinaryImage | Gets the binary image of the ChannelBase object. (Inherited from ChannelBase)
BinaryLength | Gets the length of the BinaryImageBase object. (Inherited from BinaryImageBase)
BodyImage | Gets the binary body image of the ConfigurationCellBase object. (Inherited from ConfigurationCellBase)
BodyLength | Gets the length of the BodyImage. (Inherited from ConfigurationCellBase)
DigitalDefinitions | Gets a reference to the DigitalDefinitionCollection of this ConfigurationCellBase. (Inherited from ConfigurationCellBase)
FooterImage | Gets the binary footer image of the ConfigurationCellBase object. (Inherited from ConfigurationCellBase)
FooterLength | Gets the length of the FooterImage. (Inherited from ConfigurationCellBase)
FrameRate | Gets the specified frame rate of this ConfigurationCellBase. (Inherited from ConfigurationCellBase)
FrequencyDataFormat | Gets or sets the DataFormat of the FrequencyDefinition of this ConfigurationCell. (Overrides ConfigurationCellBaseFrequencyDataFormat)
FrequencyDefinition | Gets or sets the IFrequencyDefinition of this ConfigurationCellBase. (Inherited from ConfigurationCellBase)
HeaderImage | Gets the binary header image of the ConfigurationCellBase object. (Inherited from ConfigurationCellBase)
HeaderLength | Gets the length of the HeaderImage. (Inherited from ConfigurationCellBase)
IDCode | Gets or sets the ID code of this ConfigurationCell. (Overrides ChannelCellBaseIDCode)
IDLabel | Gets or sets the ID label of this ConfigurationCellBase. (Inherited from ConfigurationCellBase)
IDLabelImage | Gets the binary image of the IDLabel of this ConfigurationCellBase. (Inherited from ConfigurationCellBase)
IDLabelLength | Gets the length of the IDLabel of this ConfigurationCellBase. (Inherited from ConfigurationCellBase)
Latitude | Gets or sets the latitude (i.e., North/South geospatial position) of the device defined by this ConfigurationCell.
Longitude | Gets or sets the longitude (i.e., East/West geospatial position) of the device defined by this ConfigurationCell.
MaximumStationNameLength | Gets the maximum length of the StationName of this ConfigurationCell. (Overrides ConfigurationCellBaseMaximumStationNameLength)
NominalFrequency | Gets or sets the nominal LineFrequency of the FrequencyDefinition of this ConfigurationCellBase. (Inherited from ConfigurationCellBase)
NumberOfSatellites | Gets or sets the number of satellites visible to the GPS timing source of the device defined by this ConfigurationCell.
Parent | Gets a reference to the parent ConfigurationFrame for this ConfigurationCell.
PhasorAngleFormat | Gets or sets the AngleFormat for the IPhasorDefinition objects in the PhasorDefinitions of this ConfigurationCellBase. (Inherited from ConfigurationCellBase)
PhasorCoordinateFormat | Gets or sets the CoordinateFormat for the IPhasorDefinition objects in the PhasorDefinitions of this ConfigurationCell. (Overrides ConfigurationCellBasePhasorCoordinateFormat)
PhasorDataFormat | Gets or sets the DataFormat for the IPhasorDefinition objects in the PhasorDefinitions of this ConfigurationCell. (Overrides ConfigurationCellBasePhasorDataFormat)
PhasorDefinitions | Gets a reference to the PhasorDefinitionCollection of this ConfigurationCellBase. (Inherited from ConfigurationCellBase)
RevisionCount | Gets or sets the revision count of this ConfigurationCellBase. (Inherited from ConfigurationCellBase)
State | Gets or sets the parsing state for the this ConfigurationCellBase. (Inherited from ConfigurationCellBase)
StationName | Gets or sets the station name of this ConfigurationCellBase. (Inherited from ConfigurationCellBase)
StationNameImage | Gets the binary image of the StationName of this ConfigurationCellBase. (Inherited from ConfigurationCellBase)
Tag | Gets or sets a user definable reference to an object associated with this ChannelBase object. (Inherited from ChannelBase)
TimeOffset | Gets or sets time offset of F-NET device in Ticks.

## See Also

#### Reference

ConfigurationCell Class
Gemstone.PhasorProtocols.FNET Namespace